Sinh Viên : Vũ Văn Trọng

Mã số sinh viên : 20184206

ASSIGNMENT 1

#Laboratory Exercise 7, Home Assignment 4

.data

Message: .asciiz "Ket qua tinh giai thua la: "

.text

main:

jal WARP

print:

add $a1, $v0, $zero # $a0 = result from N!

li $v0, 56

la $a0, Message

syscall

quit:

li $v0, 10 #terminate

syscall

endmain:

#---------------------------------------------------------------------

#Procedure WARP: assign value and call FACT

#---------------------------------------------------------------------

WARP:

sw $fp,-4($sp) #save frame pointer (1)

addi $fp,$sp,0 #new frame pointer point to the top (2)

addi $sp,$sp,-8 #adjust stack pointer (3)

sw $ra,0($sp) #save return address (4)

li $a0,5 #load test input N

jal FACT #call fact procedure

nop

lw $ra,0($sp) #restore return address (5)

addi $sp,$fp,0 #return stack pointer (6)

lw $fp,-4($sp) #return frame pointer (7)

jr $ra

wrap\_end:

#---------------------------------------------------------------------

#Procedure FACT: compute N!

#param[in] $a0 integer N

#return $v0 the largest value

#---------------------------------------------------------------------

FACT:

sw $fp,-4($sp) #save frame pointer

addi $fp,$sp,0 #new frame pointer point to stack’s top

addi $sp,$sp,-12 #allocate space for $fp,$ra,$a0 in stack

sw $ra,4($sp) #save return address

sw $a0,0($sp) #save $a0 register

slti $t0,$a0,2 #if input argument N < 2

beq $t0,$zero,recursive#if it is false ((a0 = N) >=2)

nop

li $v0,1 #return the result N!=1

j done

nop

recursive:

addi $a0,$a0,-1 #adjust input argument

jal FACT #recursive call

nop

lw $v1,0($sp) #load a0

mult $v1,$v0 #compute the result

mflo $v0

done:

lw $ra,4($sp) #restore return address

lw $a0,0($sp) #restore a0

addi $sp,$fp,0 #restore stack pointer

lw $fp,-4($sp) #restore frame pointer

jr $ra #jump to calling

fact\_end:

* Kết quả:

